KAILLERA: loaded "KailleraClient.dll" version 0.9.
APPLICATION: configuration file "D:\GAMES\SMALL\Денди\Эмуляторы\Nestopia\Nestopia.cfg" not present. using default settings
TIMER: performance counter present
DIRECTDRAW: enumerating device, guid: default, name: Первичный видеодрайвер
DIRECTDRAW: found 33 valid display mode(s) for this device
DIRECTDRAW: enumerating device, guid: 67685559-3106-11D0-B971-00AA00342F9F, name: RADEON 9600 SERIES    
DIRECTDRAW: found 33 valid display mode(s) for this device
DIRECTDRAW: creating device, guid: 00000000-0000-0000-0000-000000000000
DIRECTSOUND: enumerating device, guid: default, name: Первичный звуковой драйвер
DIRECTSOUND: enumerating device, guid: BD6DD71A-3DEB-11D1-B171-00C04FC20001, name: SB PCI
DIRECTSOUND: enumerating device, guid: C2AD1800-B243-11CE-A8A4-00AA006C4500, name: Модем №0, линейный выход (эмуляция)
DIRECTSOUND: DirectSoundCreate8() on this device failed, continuing enumeration..
DIRECTSOUND: enumerating device, guid: C2AD1800-B243-11CE-A8A4-00AA006C4501, name: Модем №0, выход трубки (эмуляция)
DIRECTSOUND: DirectSoundCreate8() on this device failed, continuing enumeration..
DIRECTSOUND: creating device - guid: 00000000-0000-0000-0000-000000000000
DIRECTSOUND: creating 8820 byte sound buffer
DIRECTSOUND: sample rate - 44100
DIRECTSOUND: sample bits - 16
DIRECTINPUT: initializing
DIRECTINPUT: found 1 attached joystick(s)
DIRECTDRAW: creating the primary surface
DIRECTDRAW: refresh rate is at 70 hz
DIRECTDRAW: creating the nes render target surface in system memory
DIRECTDRAW: surface dimensions (256,240)
DIRECTDRAW: source blit dimensions (0,8) - (256,232)
DIRECTDRAW: target blit dimensions (6,44) - (518,492)
DIRECTDRAW: filter - none
DIRECTDRAW: scale factor - 0
MACHINE: loading NES file "D:\GAMES\SMALL\Денди\Новые ромы\Crisis Force (J).nes"
MACHINE: power on
PPU: reset
MAPPER 23: reset
MAPPER 23: board name: KONAMI VRC2B
MAPPER 23: 128k PRG-ROM present
MAPPER 23: 128k CHR-ROM present
MAPPER 23: 8k WRAM present for compatibility
MAPPER 23: defaulting to horizontal PPU name-table mirroring
MAPPER 23: IRQ counter present
CPU: reset
CPU: Program Counter: 0xEA80
CPU: Stack Pointer: 0xFF
CPU: A register: 0x0
CPU: X register: 0x0
CPU: Y register: 0x0
CPU: C flag: 0
CPU: Z flag: 1
CPU: I flag: 1
CPU: D flag: 0
CPU: V flag: 0
CPU: N flag: 0
APU: reset
MACHINE: auto-changed to NTSC
DIRECTDRAW: creating device, guid: 67685559-3106-11D0-B971-00AA00342F9F
MACHINE: power off
